bits

5′GT GC GC AGA CAGAAGAAT AT TA CAGC AA CT AT GT 3′