bits

5′AT AT GT GT GT AC GT TA CT CT CAT GT CAT AT CACATACT C GT T GATC AT AT 3′