bits

5′TC AG AT AT TC GAT C AGT CT AT T TC GAC GACT GT CA GT 3′