bits

5′CGGGTGCGAAATACGACGGGC GTG TAT AT CT AGGTGGGC T AT TC 3′