bits

5′AT GT AT T AT C C TC GC AT AAGAC GGAT AAGACACT GT GT 3′