bits

5′C T AT GG GACT TGAGATAT CA3′