bits

5′C G T GAT AT TAGC TA GAC TC T ATC AT AAGC G3′