bits

5′GC AT GCA T ACT G GTC A GTA C CGT A GCTAGCTAGCAT GCTACTAGGACT GCAT GACT AGCT ACTGACGT GAC T GCT A CGA T TGC A GT CA GAC T 3′